#### Devices Configuration Wizard

1. Login as an administrator.

2. From the ribbon, choose Devices, then Setup.

3. The Device Configuration Wizard appears.

Devices Configuration Wizard dialog screen 1

3. Click the Next > button to advance to the next wizard screen.

Devices Configuration Wizard dialog screen 2

4. Select the correct device from the Please select a device drop-down list.

5. Click the Next > button to advance to the next wizard screen.

Devices Configuration Wizard dialog screen 3

6. If necessary, click on the Find <Device> button (in the above screen it's called Find GageWay) to locate and copy in the Connection Status information directly from the device.

7. Select the appropriate Device Parameters tab for the device you're connecting.

8. If using channels, update the Baud Rate, Data Bits, Parity and Stop Bits from the respective drop-down lists. Use the Copy and Paste buttons to copy these RS232 settings from one RS232 channel tab to another as necessary. Alternately, click on the Apply changes to other tabs check box if you want all the other channel tabs to use the same settings.

If using a network for communication purposes, select the Network tab. The <Device> Server options (GageWay Server in the example below) are displayed.

Device Parameters Network options

Update the TCP/IP address, Subnet Mask and Base port number as necessary.

9. Click on the Send Parameters button to test the settings with the device if necessary.

10. Click the < Back button at any time to return to the previous wizard screen.

11. If finished and all the settings test successfully, click the Finish button to store the updates and return to the DataGauge+ screen. Click the Cancel button to exit the wizard without saving the changes.