#### Port Wizard

Use this wizard to set the port type and its parameters.

1. Login as an administrator.

2. On the Configure tab, in the Communication group, click Port Management to open the Port Management dialog box.

3. To open a Port Wizard, right-click anywhere in the dialog box, and click Add.

Port Wizard - Port Type screen

4. Select the appropriate port from the Port Type list.

5. Click Next to advance to the next screen.

6. Depending on the selected Port Type in the previous screen, select or type the appropriate name.

- If Port Type is SerialPort, select the appropriate Port Name from the list.

- If Port Type is EthernetPort, type the name in the field.

Port Wizard - Port Name screen

7. Click Next to advance to the next screen.

8. If you selected SerialPort then in the Parameters screen, update the Baud Rate, Data Bits, Parity and Stop Bits from the respective drop-down lists.

If you selected EthernetPort then in the Parameters screen, update the TCP/IP address, Subnet Mask and Port number.

9. Click Back at any time to return to the previous screen.

10. Once you are done filling out the wizard, click the Finish to store the updates and return to the DataGauge+ screen. Click Cancel to exit the wizard without saving your changes.