#### Device Configuration Wizard

Use this wizard to configure the device and set the parameters.

1. Login as an administrator.

2. On the Configure tab, in the Communication group, click Setup.

Device Configuration Wizard - Welcome screen

3. Click Next to advance to the next screen.

Device Configuration Wizard - Device Selection screen

4. From the Select a device list, choose your device.

5. Click Next to advance to the next screen.

Device Configuration Wizard - Device screen

6. If necessary, click on the Find <Device> button (in the above screen it's called Find GageWay) to locate and copy in the Connection Status information directly from the device.

7. Select the appropriate Device Parameters tab for the device you're connecting.

8. If you are using channels, update the Baud Rate, Data Bits, Parity and Stop Bits from the respective drop-down lists. Use the Copy and Paste buttons to copy these RS232 settings from one RS232 channel tab to another as necessary. Alternately, click on the Apply changes to other tabs check box if you want all the other channel tabs to use the same settings.

If you are using a network for communication purposes, select the Network tab. The <Device> Server options are displayed.

Device Parameters Network options

Update the TCP/IP address, Subnet Mask and Base port number as necessary.

9. Click Send Parameters to test the settings with the device if necessary.

10. Click Back at any time to return to the previous screen.

11. Once you are finished, and all the settings test successfully, click Finish to store the updates and return to the DataGauge+ screen. Click Cancel to exit the wizard without saving your changes.