# Getting Started

To begin using PC-DMIS Gear, complete the following steps:

Step 1: Install PC-DMIS Gear

Step 2: Launch PC-DMIS Gear

Step 3: Modify PC-DMIS Gear Settings

Step 4: Create or Open a Gear File

Step 5: Calibrate Probes

Step 6: Define Gear Parameters

Step 7: Create an Alignment

Step 8: Measure the Master Flank (only used for bevel gears)

Step 9: Measure a Gear

Step 10: Review Measured Data

Step 11: Analyze a Gear

Depending on your gear type, review the following sections:

Parameters for Cylinder Gears

Parameters for Bevel Gears