## Editing Measurement Parameters for Cylinder Gears

The Gear Measurement Setup dialog box allows you to edit the parameters and begin gear measurement.

| Clicking the Measure button or selecting the Measure | Measure menu option displays the Gear Measurement Setup dialog box.

Before measuring, ensure that you have first:

- Defined your probe

- Calibrated your probe

- Defined gear parameters

- Created an alignment

See either "CMM: Gear Measurement Setup" or "Vision: Gear Measurement Setup" depending on your selected machine type.

More:

Vision: Gear Measurement Setup

CMM: Gear Measurement Setup

Defining Scan Settings

The Execute Dialog Box