## Measuring a Bevel Gear

Use the Measure Gear dialog box to edit the parameters and begin gear measurement.

To measure a bevel gear, select the Operation | Measure Gear… menu option or the Measure toolbar icon…

…to open the Measure Gear dialog box.

Before measuring, ensure that you have first:

- Defined your probe

- Calibrated your probe

- Defined gear parameters

- Created an alignment

More:

Gear Measurement Setup

Defining Scan Settings