#### Face or Root Cone Measurement Parameters

To set the Face/Root Parameters for the measurement of cone:

1. Select whether you want to measure a Face Cone or Root Cone.

2. For a Root cone you must specify the probable Tooth Height (available to edit if Root is selected).

3. Define the Number of teeth to measure.

4. If you want to move origin point to the cone apex check the Move Origin point to the cone apex option.

5. If you checked the Move origin point to the cone apex, you need to provide the Distance to Face/Root Cone from Pitch Cone apex.

6. Specify the Clearance distance from Face/Root cone for the distance you want the probe to retract after measuring each tooth.

7. Specify the Clearance distance in Z direction for the distance you want the probe to retract after measuring the entire face/root cone.

8. To accept the parameters and go back to Create Alignment dialog box, click OK. Click Cancel to close without saving changes.