### Calibrate Probes

In order to measure your bevel gear, you must first calibrate your probe.

To Calibrate you probe:

1. Select the Measure | Probe Calibration menu option...

... or the Probe Calibration toolbar icon...

... to open the Probe Utilities dialog box. PC-DMIS launches in the background to allow you to use the Probe Utilities dialog box.

2. Calibrate your probe. If needed, see the core PC-DMIS help file for information on calibrating probes.

3. Click OK when you have finished the probe calibration.