# Executing Accuracy Alignment

The Accuracy Alignment is executed when you have selected Face or Root Cone Measurement option from the Create Alignment dialog box. Otherwise the "Basic Alignment" is executed.

Some blueprints require a more accurate alignment that is created using a face/root cone.

To Execute an Accuracy Alignment:

1. Follow the instructions given in the Wizard to complete the Accuracy Alignment:

2. You will always need to take 2 hits on the face/root cone of the bevel gear, and the PC-DMIS part program for face/root cone will be built automatically.

3. Click Delete to delete the points that were just taken, if you are not stisfied with the result.

4. Click Done to measure the face/root cone.

Important: The alignment can not be undone after you click Done button.

5. Same as Basic alignment, After you have measured all points this Execution box will appear. Click Cancel to cancel the auto measure or click OK to proceed with the measurement.

6. When automatic alignment process has completed following message box will appear.

The Accuracy Alignment is now complete.