### Analyzing Gear Data

Quality Class

- Quality Type: Select the quality type from AGMA 2009, AGMA 390.03a, or DIN 3965. PC-DMIS Bevel Gear automatically determines the tolerances Fp, fp, fu and Fr from the given gear quality number and quality type and inserts these tolerances into the corresponding values (see evaluation of pitch and runout in the "Defining Pitch/Runout Data" topic). If you don't specify the gear quality the tolerances will not be determined.

- Quality Number: This number specifies the quality grade.

Analysis Options

- Topopragh: Select this option for Topography output to be created. Click Parameters to make changes to the Topography Parameters. See "Defining Topography Data".

- Pitch Runout: Select this option for Pitch/Runout output to be created. Click Parameters to make changes to the Pitch/Runout Parameters. See "Defining Pitch/Runout Data".

Plot Information

Provide Plot Information for Part Number, Notation, Serial Number, Inspector, and Machine ID that will be included in the header of your report. The Date/Time value is supplied automatically based on the time of the gear measurement.

Click this button to send your measurement data to the Quindos PageViewer. The measurement data for the measured teeth of your gear is then available in Quindos PageViewer for analysis and printing.

Click this button to close with saving any changes.

See the "Sample Pitch & Runout Report" and "Sample Topography Report" topic for examples of the reports that are created by PC-DMIS Bevel Gear.