### Install PC-DMIS Bevel Gear

To install PC-DMIS Bevel Gear:

1. Attach the portlock that is programmed with the PC-DMIS Bevel Gear option enabled. This is required to run PC-DMIS Bevel Gear.

2. Download the current version of PC-DMIS Bevel Gear from the WAI ftp-site at ftp://ftp.wilcoxassoc.com/SpiralBevelGear/ if you have not already done so. The file is named SpiralBevelGear_Setup_<version>.zip

3. Install PC-DMIS Bevel Gear by double-clicking Setup.exe. Follow the instructions given by the install wizard.