### Launch PC-DMIS Bevel Gear

| Double-click the program shortcut on the desktop to launch PC-DMIS Bevel Gear. The New File dialog box will appear automatically. Specify the name of the new file and click OK, or click Close to cancel the creation of a new file.

Creating a New File:

Select ... or click ... to open the New File dialog box. | Open the New File dialog box by selecting the File | New menu option. You can also open this dialog box by clicking the New toolbar icon.
Type the name of the new file in the Bevel Gear Name box. If the file already exists you will be prompted to verify that you want to overwrite the old file. You can also click Define Geometry Parameters to provide the Geometry Parameters for your gear. See the "Defining Geometry Parameters" topic.

Opening an Existing File:

Select ... or click ... to open the Open a bevel gear dialog box. | Open the Open a bevel gear dialog box by selecting the File | Open menu option. You can also open this dialog box by clicking the Open toolbar icon. Browse to select the needed Bevel Gear (.spb) file and click Open.