<?xml version="1.0" encoding="UTF-8"?>
<ck><di ky="0" rd="About_the_Gear_Report_Window.htm|About the Gear Report Window" ct=" About the Gear Report Window  The Gear Report window is also installed as part of  the PC-DMI ..."/><di ky="1" rd="Aligning_a_Bevel_Gear.htm|Aligning a Bevel Gear" ct="  Aligning a Bevel Gear  Use the  Align Gear   dialog box to:  	 Generate a PC-DMIS 	  ..."/><di ky="2" rd="Aligning_a_Cylinder_Gear.htm|Aligning a Cylinder Gear" ct="  Aligning a Cylinder Gear  To align a cylinder gear, select the  Operation  | Align Gear …  ..."/><di ky="3" rd="Ball_Size_Definition.htm|Ball Size Definition" ct=" Ball Size Definition  This is an imaginary ball that fits in between the teeth and touches at t ..."/><di ky="4" rd="Bevel_Gear_Measurement_Setup.htm|Gear Measurement Setup" ct=" Gear Measurement Setup   Measure Gear dialog box  Generate:  If  you select this check bo ..."/><di ky="5" rd="Clocking.htm|Clocking" ct=" Clocking  Clocking sets the positive X axis of the alignment on the symmetry point of the two p ..."/><di ky="6" rd="CMM__Gear_Measurement_Setup.htm|CMM: Gear Measurement Setup" ct="  CMM: Gear Measurement Setup  You  can use the  Measure Gear  dialog box to measure and eva ..."/><di ky="7" rd="Define_K_Chart_for_Helix_Lead.htm|Define K-Chart for Helix/Lead" ct=" Define K-Chart for Helix/Lead  The   Define K-Chart for Helix/Lead  dialog  box appears whe ..."/><di ky="8" rd="Define_K_Chart_for_Profile.htm|Define K-Chart for Profile" ct=" Define K-Chart for Profile  The   Define K-Chart for Profile  dialog  box appears when you  ..."/><di ky="9" rd="Defining_a_Bevel_Gear.htm|Defining a Bevel Gear" ct=" Defining a Bevel Gear  Use  the   Define Gear  dialog  box to define the geometric and meas ..."/><di ky="10" rd="Defining_a_Cylinder_Gear.htm|Defining a Cylinder Gear" ct=" Defining a Cylinder Gear  Use the  Define Gear   dialog box to define the geometric and measu ..."/><di ky="11" rd="Defining_Master_Flank_Data.htm|Defining Master Flank Data" ct=" Defining Master Flank Data  Measurement of the bevel gear topography requires master  flank d ..."/><di ky="12" rd="Defining_Scan_Settings.htm|Defining Scan Setttings" ct=" Defining Scan Settings  T he  Scan  Setting  dialog box appears when you click the  Scan  S ..."/><di ky="13" rd="Defining_Scan_Settings_bevel.htm|Defining Scan Settings" ct=" Defining Scan Settings  T he  Scan  Setting  dialog box appears when you click the  Scan  S ..."/><di ky="14" rd="Evaluating_a_Bevel_Gear.htm|Evaluating a Bevel Gear" ct=" Evaluating a Bevel Gear  On completion of the gear measurement,  PC-DMIS Gear can evaluate me ..."/><di ky="15" rd="Evaluating_a_Cylinder_Gear.htm|Evaluating a Cylinder Gear" ct="  Evaluating a Cylinder Gear  Use the  Evaluate Gear   dialog box to define parameters  fo ..."/><di ky="16" rd="Evaluation_Setup_Tab_Bevel_Gear.htm|Evaluation Setup Tab" ct=" Evaluation Setup Tab  Use the  Evaluation  Setup  tab to specify the plot header information  ..."/><di ky="17" rd="Evaluation_Setup_Tab_Spur_Gear.htm|Evaluation Setup Tab" ct=" Evaluation Setup Tab  Use the  Evaluation  Setup  tab to specify the plot header information  ..."/><di ky="18" rd="Example_of_Gleason_Format.htm|Example of Gleason Format" ct=" Example of Gleason Format  Following is an example of master flank data in Gleason  format. M ..."/><di ky="19" rd="FA.htm|FA" ct=" Fα  Fα  is a symbol used by your gear standard. It specifies the distance between two design pr ..."/><di ky="20" rd="Face_or_Root_Cone_Measurement_Parameters.htm|Face or Root Cone Measurement Parameters" ct=" Face or Root Cone Measurement Parameters  The  Parameters of  the face/root cone measurement ..."/><di ky="21" rd="FB.htm|FB" ct=" Fβ  Fβ is a symbol used by your gear standard. It specifies the distance between two design hel ..."/><di ky="22" rd="ffA.htm|ffA" ct=" ffα  ffα is a symbol used by your gear standard. It specifies the distance between two profiles ..."/><di ky="23" rd="ffB.htm|ffB" ct=" ffβ  ffβ is a symbol used by your gear standard. It specifies the distance between the two desi ..."/><di ky="24" rd="fHA.htm|fHA" ct=" fHα  fHα is a symbol used by your gear standard. It specifies the distance between two design p ..."/><di ky="25" rd="fHB.htm|fHB" ct=" fHβ  fHβ is a symbol used by your gear standard. It specifies the distance between two design h ..."/><di ky="26" rd="Fp.htm|Fp" ct=" Fp and fp  Fp  and  fp  are symbols used by your gear standard. They denote the  individual  ( ..."/><di ky="27" rd="Fr.htm|Fr" ct=" Fr  Fr  is a symbol used by your gear standard. It specifies the maximum amount of tooth runout ..."/><di ky="28" rd="Fu.htm|Fu" ct=" fu  fu  is a symbol used by your gear standard. It specifies the deviation between the actual m ..."/><di ky="29" rd="Gear_Options_Tab.htm|Gear Options Tab" ct=" Gear Options Tab  Use the options on the  Gear  Options  tab in the  PC-DMIS  Gear Settings ..."/><di ky="30" rd="Gear_Standard.htm|Gear Standard" ct="    Gear Standard  The four widely-used gear standards are AGMA, DIN, ISO, and JIN. While simi ..."/><di ky="31" rd="Gear_Toolbar.htm|Gear Toolbar" ct="  Gear Toolbar    Gear Toolbar  The   Gear Toolbar  has all the functionality you need t ..."/><di ky="32" rd="Getting_Started.htm|Getting Started" ct=" Getting Started  To begin using PC-DMIS Gear, complete the following  steps:  Step  1: In ..."/><di ky="33" rd="Helix.htm|Helix" ct=" Helix  This type of gear has angled teeth,instead of the teeth being straight up and down like  ..."/><di ky="34" rd="Helix_Lead_Tab.htm|Helix/Lead Tab" ct="  Helix/Lead Tab  Use  the  Helix/Lead   tab to specify the parameters for the measurement ..."/><di ky="35" rd="How_the_Report_Relates_to_the_Measured_Gear.htm|How the Report Relates to the Measured Gear" ct=" How the Report Relates to the Measured Gear  It  is helpful to understand how gear teeth are  ..."/><di ky="36" rd="Master_Flank_Measurement.htm|Master Flank Measurement" ct=" Master Flank Measurement  The following example shows the locations of the tip,  heel, root,  ..."/><di ky="37" rd="Measuring_a_Bevel_Gear.htm|Measuring a Bevel Gear" ct=" Measuring a Bevel Gear  Use the  Measure Gear  dialog box to edit the  parameters and begin g ..."/><di ky="38" rd="Measuring_a_Cylinder_Gear.htm|Measuring a Cylinder Gear" ct=" Measuring a Cylinder Gear  Use the  Measure Gear  dialog box to edit the  parameters and begi ..."/><di ky="39" rd="Menu_Options.htm|Menu Options" ct=" Menu Options  The following menu options are available in PC-DMIS  Gear.  File Menu  The  ..."/><di ky="40" rd="Normal_Diametrical_Pitch.htm|Normal Diametrical Pitch" ct=" Normal Diametrical Pitch  The diametrical pitch corresponding to the normal circular pitch and  ..."/><di ky="41" rd="Output_Settings_tab.htm|Output Settings Tab" ct=" Output Settings Tab  Use the options on the  Output  Settings  tab in the  PC-DMIS  Gear Se ..."/><di ky="42" rd="Parameters_for_Bevel_Gears.htm|Parameters for Bevel Gears" ct=" Parameters for Bevel Gears  This section provides detailed information for the  parameters th ..."/><di ky="43" rd="Parameters_for_Cylinder_Gears.htm|Parameters for Cylinder Gears" ct=" Parameters for Cylinder Gears (Spur  or Helical)  This chapter provides detailed  informati ..."/><di ky="44" rd="Parameters_Tab_Bevel_Gear.htm|Parameters Tab" ct=" Parameters Tab  Use the  Parameters   tab to define the gear&apos;s geometry parameters. Refer to  ..."/><di ky="45" rd="Parameters_Tab_Spur_Gear.htm|Parameters Tab" ct="  Parameters Tab  Use the  Parameters   tab to define the geometry parameters for the gear.  ..."/><di ky="46" rd="Parameters_Tree_Window.htm|Parameters Tree Window" ct=" Parameters Tree Window  The Parameters Tree window is a read-only window that  displays detai ..."/><di ky="47" rd="PC-DMIS_Gear_File.htm|PC-DMIS Gear File" ct=" PC-DMIS Gear File  A PC-DMIS Gear file contains information that defines a spur or bevel gear i ..."/><di ky="48" rd="PC-DMIS_Gear_Introduction.htm|PC-DMIS Gear: Introduction" ct=" PC-DMIS Gear 2.5:  Introduction   PC-DMIS™ Gear is a completely  independent software pac ..."/><di ky="49" rd="PC-DMIS_Gear_Modes.htm|PC-DMIS Gear Modes" ct=" PC-DMIS Gear Modes  PC-DMIS Gear has two modes: Programmer Mode and Operator  Mode. If this i ..."/><di ky="50" rd="PC-DMIS_Gear_User_Interface.htm|PC-DMIS Gear: User Interface" ct=" PC-DMIS Gear: User Interface  User interface elements for PC-DMIS Gear are discussed  in the  ..."/><di ky="51" rd="PC-DMIS_Options_Tab.htm|PC-DMIS Options Tab" ct=" PC-DMIS Options Tab  Use the options on the  PC-DMIS  Options  tab in the  PC-DMIS  Gear Se ..."/><di ky="52" rd="PC_DMIS_Gear.htm|PC-DMIS Gear" ct=" PC-DMIS Gear  PC-DMIS  Gear: Introduction  Getting  Started  Step  1: Install PC-DMIS ..."/><di ky="53" rd="Pitch.htm|Pitch" ct=" Pitch  This can generally be considered as the &quot;average&quot; radius of the gear located between the ..."/><di ky="54" rd="Pitch_Runout_Tab_Bevel_Gear.htm|Pitch/Runout Tab" ct="  Pitch/Runout Tab  Use the  Pitch/Runout   tab to specify the required data for the  pitch ..."/><di ky="55" rd="Pitch_Runout_Tab_Spur_Gear.htm|Pitch/Runout Tab" ct="  Pitch/Runout Tab  Use  the  Pitch/Runout  tab to specify  the parameters for the measure ..."/><di ky="56" rd="Probe_File.htm|Probe File" ct=" Probe File  A probe file defines your current probe configuration so that PC-DMIS Gear can unde ..."/><di ky="57" rd="Profile.htm|Profile" ct=" Profile  The profile of a gear tooth from tip to root.  	   	 	    ..."/><di ky="58" rd="Profile_Tab.htm|Profile Tab" ct="  Profile Tab  Use the  Profile  tab to specify the parameters  for the measurement and eval ..."/><di ky="59" rd="Runout.htm|Runout" ct=" Runout  The Runout value can be determined theoretically by placing balls of a specified diamet ..."/><di ky="60" rd="Sample_Pitch_&amp;_Runout_Report.htm|Sample Pitch &amp; Runout Report" ct=" Sample Pitch &amp; Runout Report  The Pitch/Runout report for the spiral bevel gear is  represent ..."/><di ky="61" rd="Sample_Pitch_Runout_Layout.htm|Sample Pitch Runout Layout" ct=" Sample Pitch Runout Layout  (A) Deviation values are indicated in microns. (B)  Red arrow ind ..."/><di ky="62" rd="Sample_Profile_Helix_Measurement_Evaluation.htm|Sample Profile &amp; Helix Measurement Evaluation" ct=" Sample Profile &amp; Helix Measurement Evaluation  (A) Deviation values are indicated in microns. ( ..."/></ck>