#### Executing a Basic Alignment

A Basic Alignment is executed when you have not selected Face or Root Cone Measurement option from the Create Alignment dialog box. Otherwise the "Accuracy Alignment" is executed.

To Execute a Basic Alignment:

1. Follow the instructions given in the Wizard to complete the Basic Alignment:

2. After each measurement you can click Next to continue to the next measurement.

3. If you are not satisfied with the step that you just completed you can click Back to go to the last step. Also before you go to the next step the Back button will display as Delete; click it to delete the feature you just measured.

4. During measurement, if the hit point you have taken is not good enough to fit a feature needed, the software will warn you to remeasure it. You can click OK and continue.

Note: The last step can always be undone!

5. After you have measured all alignment features this Execution box will appear. Click Cancel to cancel the auto measure or click OK to proceed with the measurement.

6. When automatic alignment process has completed following message box will appear.

7. The Basic Alignment is now complete.