### Menu Options

The following menu options are available in PC-DMIS Bevel Gear:

File Menu

- New: Create a new Bevel Gear file.

- Open: Open an existing Bevel Gear file. You will be prompted to save your work before the current file is closed and the selected file is opened.

- Close: Close the current Bevel Gear file.

- Save: Save the current Bevel Gear file with the current file name and file type (*.bevel).

- Save as: Save the current Bevel Gear file with a specified name.

- Language: Select the language that will be used for the PC-DMIS Bevel Gear application.

- Exit: Exit PC-DMIS Bevel Gear.

Measure Menu

- Measure: Measure your gear. See "Measure a Gear".

- Analyze: Analyze the measured results for your gear. See "Analyze Measured Data and Create Report".

- Master Flank: Measure the Master Flank to create a Gleason file. See "Measure the Master Flank".

- Modify Geometric Parameters: Set geometry parameters for your gear. See "Modifying Geometry Parameters".

- Probe Calibration: Calibrate your Probe. See "Calibrating Your Probe".

- Alignment Creation: Create alignment for the gear you want to measure. See "Editing Alignment Values".

- Data Viewer: View the nominal and actual data for your measured gear. See "Viewing Feature Data".

- Browse Data Folder: Open the Data folder inside the PC-DMIS Bevel Gear install directory.

- Create Log File: Selecting this option will cause debug information to be collected for troubleshooting problems. Debug information is stored in the BvGear.log file in the PC-DMIS Bevel Gear install directory.

View Menu

- View Menu Items: Toggles the display of the respective SBG application elements: Parameters Tree Window, Status Window, Statusbar, & Toolbar.

Help Menu

- Contents and Index: Open the PC-DMIS Bevel Gear help file.

- About PC-DMIS BevelGear: Displays information about your version of PC-DMIS Bevel Gear.