### Face or Root Cone Measurement Parameters

The Parameters of the face/root cone measurement dialog box appears when you select the Parameter setup button in the Align Gear dialog box.

Parameters of the face/root cone measurement dialog box

To set the face cone or root cone parameters for the measurement of the cone:

1. Select the Number Of Teeth to measure.

2. Select whether you want to measure a Face Cone or a Root Cone.

3. If you selected Root Cone, the Tooth Height box becomes available. Specify the tooth height.

4. If you want to move the origin point to the cone apex, select the Move origin to the cone apex option.

5. The Distance To Face/Root Cone From Pitch Cone Apex box is available if you selected the Move origin to the cone apex option.

6. For Clearance Distance From Face/Root Cone, enter the distance you want the probe to retract after measuring each tooth.

7. For Clearance Distance In Z Direction, enter the distance you want the probe to retract after measuring the entire face cone or root cone.

8. To accept your changes, click OK. To close without saving your changes, click Cancel.