### Toolbar

1. New: Create a new Bevel Gear file.

2. Open: Open an existing Bevel Gear file. You will be prompted to save your work before the current file is closed and the selected file is opened.

3. Close: Close the current Bevel Gear file.

4. Save: Save the current Bevel Gear file with the current file name and file type (*.spb).

5. Probe Calibration: Calibrate your Probe. See "Calibrating Your Probe".

6. Alignment Creation: Create alignment for the gear you want to measure. See "Editing Alignment Values".

7. Measure: Measure your gear. See "Measure a Gear".

8. Analyze: Analyze the measured results for your gear. See "Analyze Measured Data and Create Report".

9. Modify Parameters: Set geometry parameters for your gear. See "Modifying Geometry Parameters".

10. Create Master Flank: Measure the Master Flank to create a Gleason file. See "Measure the Master Flank".

11. Browse Data Folder: Open the Data folder inside the PC-DMIS Bevel Gear install directory.

12. Change Language: Click the small arrow next to the icon and select the language that will be used for the PC-DMIS Bevel Gear application.

13. Help: Open the PC-DMIS Bevel Gear help file. Click the arrow next to this icon and select either "Contents and Index" to open the help file, or select "About PC-DMIS BevelGear" to view Application build information.