## Measuring a Cylinder Gear

Use the Measure Gear dialog box to edit the parameters and begin gear measurement.

To measure a cylinder gear, select the Operation | Measure Gear… menu option or the Measure toolbar icon…

…to open the Measure Gear dialog box.

Before measuring, ensure that you have first:

- Defined your probe

- Calibrated your probe

- Defined gear parameters

- Created an alignment

See either "CMM: Gear Measurement Setup" or "Vision: Gear Measurement Setup" depending on your selected machine type.

More:

Vision: Gear Measurement Setup

CMM: Gear Measurement Setup

Defining Scan Settings

The Execute Dialog Box