### User Tolerance Chart

The User Tolerance Chart screen lets you specify tolerances for future recall in the Tolerance screen of any feature by using the Select Global Tolerance Limit list located in that screen. This provides you with a rapid way of selecting and entering the same tolerance values repeatedly.

To define user tolerances:

1. Touch the Setup soft key from the main screen.

2. Then touch the Define Tolerance Chart soft key.

3. For the desired TC classes, type the +Limit or -Limit tolerance values.

4. Once you have TC classes defined touch Apply Changes. You can then select these TC classes from the Tolerance screen.