#### Set Work Offsets

Setting work offsets lets you update the work offset on the controller by measuring a selection of features.

1. From the main screen, choose the Set Work Offsets soft key. The soft keys at the bottom will change to show the different types of features you can measure to set a work offset:

2. Touch the desired measurement procedure:

- Update One Axis

- Update Two Axes (Bore)

- Update Two Axes (Boss)

- Update Two Axes (Inside Corner)

- Update Two Axes (Outside Corner)

3. The appropriate screen will appear.

Note: You can also update a work offset by using the Update Work Offset screen.

Available Navigation Bar Soft Keys on this Screen:

| Backward When enabled, this soft key scrolls back to any additional buttons available on the first page for this screen. |  | Update One Axis This soft key accesses the 'Update One Axis' screen.
| Update Two Axes (Bore) This soft key accesses the 'Update Two Axes (Bore)' screen. |  | Update Two Axes (Boss) This soft key accesses the 'Update Two Axes (Boss)' screen.
| Update Two Axes (Inside Corner) This soft key accesses the 'Update Two Axes (Inside Corner)' screen. |  | Update Two Axes (Outside Corner) This soft key accesses the 'Update Two Axes (Outside Corner)' screen.
| Help This soft key accesses the NC Gage help file. |  | Return This soft key returns the view up one level to the previous screen.
|  |  | Forward When enabled, this soft key scrolls forward to any additional soft keys available on the second page for this screen.