### Construct Point

1. Select the Measure soft key from the main screen's Navigation Bar.

2. Select the Forward soft key until you get to the third page of soft keys.

3. Select the Construct a Point soft key from the Navigation Bar. The Construct Point screen appears.

This screen lets you create a point feature by doing one of the following:

- Constructing a point at the intersection of two selected line type features.

- Constructing a point by projecting a point type feature onto a line type feature.

- Constructing a point midway between two selected point type features.

To Construct a Point Feature

1. From the Option area, select the option button for the type of construction to take place.

2. Select the appropriate work face.

3. Select the two features. Only the valid feature types will show up in the selection screen. The graphics in the upper left corner of the screen will update to provide a visual cue as to how the feature will be built. The nominal and measured data will update according to the feature inputs.

4. Press the Confirm soft key to add the command to the program.

Valid Point Type Features: | Valid Line Type Features:

- Circle Bore

- Circle Boss

- Corner Inside

- Corner Outside

- Constructed Points

- Web

- Pocket

- Line

- Constructed Lines

Available Navigation Bar Soft Keys on this Screen:

| Backward / Forward Back / Forward to previous / next group of soft keys. |  | Select Measurement Face This soft key determines the direction of probing and the location of the clearance moves for the feature. You can press this multiple times to choose a different measurement face. Available faces are: X+, X-, Y+, Y-, Z+ and Z-.
| Delete Current Command / Delete Last Created This soft key deletes the current selected command (or the last created command) from the part program. If this icon is disabled, you may need to delete commands using the Edit Program screen instead. |  | Confirm / Add Command For operations this confirms the selection. For commands, this will append the command to the end of the program. For feature commands, this will become available after the machine has learned the feature location or when you have typed the feature's nominal values.
For constructed and dimension feature commands, this will become available once you have specified the proper input features.

| Insert Command after Current Position This soft key adds the command into the part program but places it after the selected command in the program tree instead of at the end of the program. |  | Cancel All Steps / Abort This soft key stops and resets the current operation. If learning a feature, it removes all the learned probe positions.
| Help This soft key accesses the NC Gage help file. |  | Tolerance Settings This soft key lets you set or modify feature nominal and tolerance values used by the feature command. It is an overview of what will show up in the report screen.
| Return This soft key returns the view up one level to the previous screen. |  |