To get running with the simulator, run Measure.exe. This is the simulator. Then run NcGage.exe. Add a probe, use probe pocket 1 for the probe, use probe diameter/size/tip of 6, probe length of 10. Calibrate the probe using Sphere. The sphere diameter for calibration sphere screen is 25. Center is X Y Z is 100, 0, 150 (for center of sphere).

## Introducing NC Gage

PC-DMIS NC Gage version 2.0 provides an easy-to-use product for online part measurement using NC machine tools. NC Gage can enhance your machine part productivity and precision by providing you with a simple user interface that allows you to easily insert needed feature measurements and other commands in your part program.

Terminology Note: Since many users run NC Gage on a touch screen display, the terms "select" or "press" used in this documentation indicate a mouse click when running the software on a PC with mouse and keyboard peripherals attached.

This documentation discusses the following main topics:

- Configuration

- Getting Started

- Creating Feature Commands

- Setting Additional Feature Parameters

- Inserting Move Commands

- Working with Programs

- Using Reports

- Direct Connect Mode

- Controller Configuration

Help File Last Updated: May 5, 2011