### Calibration Values Test (Calibration Test Settings)

This screen will allow the user to indicate the nominal location of the ring and tolerance values. If any measured value differs from its respective nominal by more than the allotted tolerance, a warning will be displayed. The user will be able to continue after accepting the warning. The nominal X, Y, and Z can be entered. The tolerances for the X, Y, Z, D, and form (F) can be entered.