#### Write Rotary Calibration Data To Control

The Write Rotary Calibration Data to Control option is used after the rotary table(s) have been successfully calibrated to send the calibration information to a block of macro variables of the controller.

1. Press the Probe soft key from the Main screen to access the Probe options screen.

2. Press the Write Rotary Calibration Data To Control soft key to display the following screen.

3. Enter the first macro variable number (for Center X of Base Table). The remaining macro variable numbers will be assigned sequentially.

4. Press the Confirm soft key to transfer the calibrated values to the controller. The macro variable numbers will fill in sequentially as shown below. It is up to the user to appropriately apply these values on the controller end.