## Rotary Table Options

When defining a measuring system that uses rotary tables, the nominal location and orientation of the rotary table(s) must be entered.

Calibration may optionally be performed to increase the accuracy of the measurements when the tables are used as part of a measurement sequence.

The Rotary Table Calibration feature is available from the Probe options screen.

To access the Probe options screen:

1. Press the Probe soft key from the Main screen to access the Probe options screen.

2. Press the Rotary Table Calibration soft key to calibrate the rotary table(s) in your system.

The following optional methods can be found on the Rotary Table Calibration screen:

- View Calibration Report soft key used to view the calibration report after successfully calibrating your rotary table(s).

- Find Sphere Tool soft key used to define the sphere being used to calibrate the rotary table(s) in your system.

The following optional methods are available from the Probe options screen:

- Select a Probe soft key used to select or define a new probe to be calibrated.

- Sphere Calibration soft key used to calibrate the probe in your system using a Calibration Sphere.

- Ring Calibration soft key used to calibrate the probe in your system using a Calibration Ring.

- Probe Length Refinement soft key used to calculate the length of your probe.