#### Set Work Offsets

Setting work offsets lets you update the work offset on the controller by measuring a selection of features.

1. Press the Set Work Offsets soft key from the Main screen. The soft keys at the bottom will change to show the different types of features you can measure to set a work offset:

2. Click on the a specific measurement procedure from the following:

- Update One Axis

- Update Two Axes (Bore)

- Update Two Axes (Boss)

- Update Two Axes (Inside Corner)

- Update Two Axes (Outside Corner)

- Update Three Axes With Sphere

- Update Rotary Axes (Angle)

3. The appropriate screen will appear.

Note: You can also update a work offset by using the Update Work Offset screen.

Available Navigation Bar Soft Keys on this Screen:

| Update One Axis This soft key accesses the 'Update One Axis' screen. |  | Update Two Axes (Bore) This soft key accesses the 'Update Two Axes (Bore)' screen.
| Update Two Axes (Boss) This soft key accesses the 'Update Two Axes (Boss)' screen. |  | Update Two Axes (Inside Corner) This soft key accesses the 'Update Two Axes (Inside Corner)' screen.
| Update Two Axes (Outside Corner) This soft key accesses the 'Update Two Axes (Outside Corner)' screen. |  | Set Three Axes With Sphere Used to measure a sphere and then use the measured coordinates to update a specified work offset.
| Set Rotation Axes Angle With Line Used to define and display all features that generate a well defined angle in the rotary axis plane. |  |