## Recommended System Requirements

- PC-DMIS NC Gage operates under Windows XP 32-bit or Windows XP 64-bit (x64) Operating System or higher (Vista, Win7).

- 2 GHz or higher Intel Pentium 4 or higher processor recommended

- 500 Mb of RAM or higher

- 500 Mb of free hard drive space

- SVGA graphics card capable of OpenGL shading with at least 64 MB Video RAM and WHQL (Microsoft Windows Hardware Quality Labs) certified drivers. (WHQL drivers can be downloaded automatically when using the Windows Update software.)

- Microsoft .NET 2.0

- SVGA capable monitor

- Screen resolution of 1024 x 768 or higher

- 2 USB Ports

Controller Requirements:

- 100 Kb free memory

- 35 available registry variables

- If Fanuc based controller - Focus B Support, High Speed Skip, and an Ethernet connection

ANTI-VIRUS SOFTWARE: The Sophos Anti-virus tool was used by Hexagon Metrology while testing PC-DMIS NC Gage. The performance of any other anti-virus tool will need to be confirmed by the user.

http://sophos.com/products/enterprise/endpoint/security-and-control/