## About the Blade Scan Profile Command

You can use the Blade Scan Profile command to create the profile dimension of each blade section in order as required by BladeRunner. The Blade Scan Profile command will automatically search for all Blade Scan commands in the part program and create a list of the concave (CC) and convex (CV) sections. The command will output Surface Profile dimensions with the “Form and location” control option and Textual Analysis enabled as required by BladeRunner.

Note the following:

- The Blade Scan Profile command supports the requirements of BladeRunner. BladeRunner requires every section to be measured as CC and CV sides. Each side is reported in order. Therefore, the Blade Scan Profile command creates profile dimensions for only those sections that have been programmed to measure the CC and CV sides.

- If you selected Both for the Side option in the Blade Scan dialog box to scan both sides of a blade section, the Blade Scan Profile command will divide the complete section into two parts and report them as CC and CV so that BladeRunner can support it.