PC-Dmis 2010 Object Library | Send comments on this topic. | See Object Hierarchy Chart
ControlPoint Object Members
See Also Overview

Collapse All Expand All

# Public Properties

Crossings | Read/Write: Number of Crossings for control point This defines the number of time the scan crosses the specified boundary before the alterations defined by the crossing point take effect.
I | Read/Write: I component of control point vector This specifies the I component of the interrupt location's IJK vector.
J | Read/Write: J component of control point vector This specifies the J component of the interrupt location's IJK vector.
K | Read/Write: K component of control point vector This specifies the K component of the interrupt location IJK vector.
PointDensity | Read/Write: Number of Points per MM for control point This defines the density of points per millimeter the scan shoud take after it encounters the control point.
PointDensity2 | Read/Write: Number of Points per MM for control point. Can be less than 1
Radius | Read/Write: Radius of control point (Sphere/Cylinder) This defines the Radius of circular control point types (Cones, Spheres, Cylinders).
Speed | Read/Write: Scan Speed Setting for control point
Type | Read/Write: Type of scan control point This specifies the type of control point.
X | Read/Write: X component of control point location This specifies the X value of the interrupt XYZ location.
Y | Read/Write: Y component of control point location This specifies the Y component of the interrupt XYZ location.
Z | Read/Write: Z component of control point location This specifies the Z component of the interrupt XYZ location.

# See Also

ControlPoint Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.