### Mount Point

Probe Changer dialog box—Mount Point tab

The Mount Point tab allows you to change the values for the AB wrist angle as well as define a safe position that the CMM can move to before each change cycle.

You can do this for as many probe changers as defined using the Type tab. Select the probe changer from the Active Probe Changer list and type the desired AB angles and machine position.

More:

Active Probe Changer

Probe Head Wrist Angle

Machine Position