### To Apply True Position on a Group of Circles or Cylinders

1. Create a feature set of the holes from the Insert | Feature | Constructed | Set menu option (see "Constructing a Set of Features" from the "Constructing New Features from Existing Features" section for instructions on creating feature sets.).

2. Select the True Position menu option. The True Position dialog box appears.

3. From the True Position dialog box, select the created feature set as the input feature, and select any other options used for the dimension.

4. Select the Textual check box from the Analysis area.

5. Access the Report window (View | Report window) and from the Reporting toolbar, select the View Report Mode icon. You are now able to see the deviation of each feature and the translation and rotation required to bring the features into tolerance. Results are always shown using Regardless of Feature Size (RFS ) on Datum to see the maximum deviation.