#### Mitutoyo Interface tab

Machine Options dialog box - Interface tab

The Interface tab allows you to configure the following settings for the Mitutoyo interface.

PH9 - Select this option if you are using a PH9.

Old Joystick - If the Jog box is an old type then this option must be set to 1. (If the jog box functions do not perform as set out below then you have an old joy stick)

BHN 706 - Select this option if you are connecting to a BHN 706 CMM.

Top Speed - This sets the overall top speed for the machine. If this value is too high then you will get intermittent ‘overspeed’ errors from the controller during DCC moves. Default is 60.

In Position Tolerance - This is the value that sets how close the machine has to get to a commanded position before it accepts that it is there. If the machine seems to pause between moves for excessive time then you could try increasing this value.

Caution: These values should only be changed by a trained technician. Altering these values may give an undesired result.