#### Start Label

The Start Label box allows you to define a label that PC-DMIS will go to when remeasuring iterative alignment features as long as you select the Meas All Always check box.

- PC-DMIS will re-measure in DCC mode, starting at the designated label and ending at the ALIGNMENT/START command (preceding the ALIGNMENT/ITERATE command). This is more consistent with how DMIS expects this command to function.

If you don't define a start label,

- PC-DMIS goes to the first feature making up the iterative alignment and begins DCC measurement there (PC-DMIS also includes any moves just before this feature).

- PC-DMIS will continue to re-execute part program commands in order until it reaches the last feature making up the iterative alignment. If there are any moves after this ending feature, they will not be executed.

To create a label, see "Creating Labels" in the "Branching by Using Flow Control" section.