### MLB-190 Too much probe deflection

The analog probe is over-deflected during a scan move command.

Effect

SMP is put into manual mode when:

- TrapScanDeflectStatus = False (System Default). The command is temporarily halted until SMP is put into automatic mode.

- TrapScanDeflectStatus = True. The command is not executed. The variable ScanDeflectStatus equals 2.

What you should do

1. Check part surface.

2. Check current soft probe deflection value.

3. Initiate user-generated scan error recovery routine.