### Bright Interface

The Bright interface is used with Mitutoyo Euro C (Bright) machines. This interface communicates to the controller through a proprietary card developed by Mitutoyo. If this installation is using a new PC, then the card must be removed from the original machine and put in the new one. If the customer needs to be able to still use their old software together with PC-DMIS, they both must be installed on the same machine.

Before starting PC-DMIS, rename the bright.dll to interfac.dll.

The Machine Option dialog box has two tabs for the Bright interface:

Axis tab

See the "Assigning the Machine Axes" topic.

Debug tab

See the "Generating a Debug File" topic.

Note: Additional information for this interface is provided in the Machine Interface Installation Manual (MIIM).