#### Adding Hit Lines

To add a hit line, place the cursor in the desired location and press the ENTER key. Begin by typing the command HIT. Press the TAB key. PC-DMIS adds the new line depending on where the cursor is located. If the cursor is in the middle of a command, a new line is created below the current line. If the cursor is placed anywhere within the first four lines PC-DMIS will create the new line immediately after the measured line.