### Setup Options: NC-100 Setup tab

SetUp Options dialog box—NC-100 tab

The NC-100 tab (Edit | Preferences | Setup) allows you to use a NC-100 video probe. Once the Use NC-100 Video Probe check box is selected, the TCPIP Address, Port Number, and Computer Name boxes become available. Use these boxes to set up communication settings with the NC-100 computer system. These values are stored in the registry settings and are recalled each time you start PC-DMIS. See the "Modifying Registry Entries" section.

For information on using the NC-100 Video Probe to create Auto Features, see the appropriate section in the PC-DMIS Vision documentation.

Note: The NC-100 tab only appears in PC-DMIS if your portlock is programmed to accept CMT functionality.

Item | Description
Use NC-100 Video Probe check box | The Use NC-100 Video Probe check box determines if PC-DMIS is using the NC-100 video probe. If you select this check box, PC-DMIS assumes that the NC-100 is active.
TCPIP Address box | Use the TCPIP Address box to enter the address information for the NC-100 computer system. This value is required for the communication between the PC-DMIS computer system and the NC-100 computer system.
Port Number box | Use the Port Number box to enter the port number of the NC-100 computer system. This value is required for the communication between the PC-DMIS computer system and the NC-100 computer system.
Computer Name box | Use the Computer Name box to type the name of the NC-100 computer system. This value is required for the communication between the PC-DMIS computer system and the NC-100 computer system.