####

#### Step 1 - Select the FCR25 Probe Changer

To begin the calibration process, select Edit | Preferences | Probe Changer to open the Probe Changer dialog box.

Probe Changer dialog box - Type tab

To select the FCR25 Probe Changer, follow these steps:

1. Select the Type tab from the Probe Changer dialog box.

2. Select FCR25 from the Probe Changer Type list.

3. Click Apply to make this probe changer active and to load settings that are relevant to this probe changer.

4. Specify the number of different types of probe changers in the Number of Probe Changers box.

5. Specify the Docking Speed. The default value of 5% is appropriate for most machine configurations.

6. Click Apply to save your changes.

In the next step you will define the location your probe body will move to when using the probe changer to switch probe components.

Next Step...