#### Metromec tab

Machine Options dialog box - Metromec tab

The Metromec tab allows you to configure the following settings for the Metromec interface.

PH9 - Select this option if you are using a PH9.

Max Speed - This option sets the maximum speed for your CMM.

Acceleration - This option sets the maximum acceleration for your CMM.

XYZ Mechanical Offset - These values allow you to establish the mechanical offset for your machine. This should only be adjusted by a trained technician.

Compensation Data - When you are using the DEA compensation types the compensation data file (typically compens.dat) is specified in this box. When using the new DEA comp there are three text files that must be in the PC-DMIS directory: FZYFILE.TXT, RCXFILE.TXT, and RMXFILE.TXT.

Compensation Type - Select from the following Volcomp methods: NONE, DEA Standard, or DEA DLL (wcompens32).

Compensation Mode - Select from the following supported compensation modes for the DEA DLL (wcompens32) Compensation type: Standard Machine, Horizontal Arm (Arm 1), or Horizontal Arm (Arm 2).

Caution: These values should only be changed by a trained technician. Altering these values may give an undesired result.