Current Help System: PC-DMIS CMM (View Core Help)

#### Notes on SP600 Lower Matrix:

The lower matrix procedure now uses the AP_COMP methodology developed by Brown and Sharpe Engineering. Three new settings were created and made available in the PC-DMIS Settings Editor, under the ANALOG_PROBING heading. These are:

SP6MTXMaxForce=0.54

SP6MTXUpperForce=0.3

SP6MTXLowerForce=0.18

The values given to these settings are those currently recommended by Brown and Sharpe Engineering during the lower matrix procedure. These entries will be created (if they don't already exist) the first time you run the lower matrix procedure.

You shouldn't change these values unless Brown and Sharpe Engineering issues new recommendations in the future. The lower matrix procedure will use these settings regardless of any OPTIONPROBE command that may or may not be present in the current part program.

For information on the PC-DMIS Settings Editor, see the "Modifying Registry Entries" documentation.

For additional information on the Lower Matrix procedure, follow the link to the SP600 Low Level Matrix document located on the Wilcox Associates, Inc. web site here:

http://www.wilcoxassoc.com/Downloads/dl_instructionalfiles.htm