Current Help System: PC-DMIS Laser (View Core Help)

#### To Position Your Laser Probe

1. Adjust the Increment Value in the Increment edit box to specify the amount that the Current Position edit box will be increased or decreased.

2. Click the Up and Down arrows to change the value in the Current Position edit box . This will cause your Laser Probe to move in real time by the specified value. Alternately, you may type the value and hit enter to cause your Laser Probe to move.