Current Help System: PC-DMIS Laser (View Core Help)

### Executing Scan-Extracted Auto Features

When executing manual scans from which Auto Features will be extracted, you should do the following:

When executing manual scans with the extracted Auto Features, you should do the following:

1. Scan the Auto Features in you part program in any order. This can be accomplished with one or more passes. After the first pass, if the scan’s Pointcloud points have changed for a feature, then the feature's measured values will be recalculated.

2. When all the Auto Features associated with the scan have solved successfully, the command in the Edit Window will be highlighted in yellow.

3. When Auto Features have solved and have been reported correctly, the command in the Edit Window will be highlighted in green.

4. If additional scan data is taken for a feature that has already been solved, the feature's measured values will be updated again with the new solution.

5. Once all of the included Auto Features have been solved, you may choose to continue scanning to further refine the measured results or you can click the Scan Done button from the Execution Mode Options dialog box. This may also be accomplished by pressing the done button on your arm.

Note: The Scan Done button will not be available until all the included Auto Features have been measured successfully.

See the "Using Pointclouds".