NAME=CCD
Charge Coupled Device - This is one of the two main types of image sensors used in digital cameras.
NAME=Cloud of Points
The Cloud of Points command is a container for XYZ coordinate data. The data can be input from an external file, or it can come directly from a laser sensor through the referring scan command(s).
NAME=COP
The Cloud of Points command is a container for XYZ coordinate data. The data can be input from an external file, or it can come directly from a laser sensor through the referring scan command(s).
NAME=Exposure
This parameter controls the exposure of the Laser sensor.
NAME=Overscan
This parameter controls how far beyond the nominal feature’s dimensions the probe will scan along both the major and minor axis of the feature.
NAME=Row Overlap
This parameter controls how far each pass will overlap with the previous pass.
NAME=Sensor Frequency
This parameter controls the internal sensor frequency of the probe. The value that is displayed is sensor pulses per second.
