Current Help System: PC-DMIS Laser (View Core Help)

### Face Colormap COPOPER

Pointcloud Operator dialog box - Face Colormap Operator

The CAD model is shaded according to the deviations of the cloud of points compared to CAD using the colors defined in the Edit Dimension Color dialog box and the tolerance limits specified in the Tol. Up and Tol. Down boxes below.

The colors used for the color map are defined in Edit Dimension Color dialog box, which is accessed by clicking Edit | Graphics Display Window | Dimension Color.

You can view the color scale from the Dimensions Colors window by selecting the View | Other Windows | Dimensions Colors menu item.

Applying the Face Colormap operation to a Pointcloud can be done by clicking the Pointcloud Surface Color Map button from the Pointcloud toolbar or by selecting the Insert | Pointcloud | Surface Colormap menu item.

The Face Colormap Operator uses the following options:

Tol. Up - Upper tolerance value

Tol. Down - Lower Tolerance value

Refine Factor - Adjust this value to improve Colormap display

Max Distance - This value allows to discard the effect on the colormap of points located at a distance greater than the specified Max Distance.

No Data Color - When this option is selected, the specified color will be mapped to the surface where there is no data.

Clicking Create inserts a COPOPER/FACE COLORMAP command into the Edit Window like the following examples:

COPOPER6 =COPOPER/FACE COLORMAP,PLUS TOLERANCE=0.300,MINUS TOLERANCE=0.100

REF,COP1,