Current Help System: PC-DMIS Portable (View Core Help)

### Bundle Alignment Command Text

BUNDLE ALIGN/ID = 1,SHOW DETAIL = TOG1

FIT OPTIONS/TYPE = TOG2,BALANCED = TOG3,BLUNDER ANALYSIS = TOG4

MEASURE FEATURES/PNT1,PNT2,PNT3,

BUNDLED FEATURES/

STATION = 1,PNT1,PNT2,PNT3,PNT4,

STATION = 2,PNT1,PNT2,PNT3,,

STATION = 3,PNT1,PNT2,PNT4,,

STATION =

- ID: This field provides the active station number. This is the station from which "Bundle Alignment Features" will be measured.

- TOG1 (SHOW DETAIL = YES/NO): When this value is set to YES, a detailed listing of the Bundle Alignment is displayed in the Edit Window. By default, this value is set to NO, which will not display the FIT OPTIONS.

- TOG2 (FIT OPTIONS/TYPE = type): Choose one of four available Fit Options: NORMAL, POINTS AND STATIONS FIXED, RECALCULATE ALL, and STATIONS FIXED. See "Setting Fit Options".

- TOG3 (BALANCED = OFF/ON): When this value is set to ON, a balanced network solution is used. By default, this value is set to OFF. See "Setting Fit Options".

- TOG4 (BLUNDER ANALYSIS = OFF/ON): When this value is set to ON, Blunder Analysis is used. By default, this value is set to OFF. See "Setting Fit Options".

- MEASURE FEATURES: Lists "Bundle Alignment Features" that will be measured for the active station number.

- BUNDLED FEATURES: Lists stations and the "Bundle Alignment Features" that are included in the Bundle Alignment computations.