NAME=6DoF
Six Degrees of Freedom
NAME=ADM
Absolute Distance Meter
NAME=Birdbath
Your reflector can be attached to this known position via a magnetic connector located on the front of the laser tracker.
NAME=DRO
Display Readout
NAME=ID
Inside Diameter
NAME=IFM
Interferometer
NAME=Nivel
Inclination sensor designed to be used with Leica Laser Tracker. This device attaches to the laser tracker to establish orientation to gravity or monitor tracker stability.
NAME=Normal Hit
A "Normal Hit" is taken when press and release the hit button in the same location.
NAME=OD
Outside Diameter
NAME=Pulled Hit
Changes the vector to that of the line between the location where you first depress the hit button (at the "Normal Hit" location) to the location where you release the hit button. This line must be longer than the Use Vector Distance to successfully register a "Pulled Hit".
NAME=RMS
Root Mean Square
NAME=TCU
Tracker Control Unit
NAME=TTP
Touch-Trigger Probe
