Current Help System: PC-DMIS Portable (View Core Help)

### Other PC-DMIS Menu Items

Operation Menu

End Feature (END): Tells PC-DMIS that the amount of hits for the feature has been reached and the feature can be calculated.

Erase Hit (ALT+-): Deletes the last measured hit.

Take Hit (CTRL+H): Measures a stationary T-Probe or Reflector position, based on the measuring time specified in the "Sensor Configuration tab" of the Machine Options dialog box.

Start/Stop Continuous Mode (CTRL+I): Starts/Stops a scan, based on the basic scan settings found on the Part/Machine tab of the SetUp Options dialog box (Edit | Preferences | Setup). The default value for Scanning Min Distance Delta provides a continuous distance separation of 2mm.