Current Help System: PC-DMIS Settings Editor (View Core Help)

### Origin Mode

This option specifies what will be calibrated as part of the multiple arm calibration process.

- When this option is set to 0, PC-DMIS creates a 3D transformation between the two arms to compensate for any out-of-squareness between the two arms. You must do this at least once (normally this is done periodically every few months).

- When this option is set to 1, PC-DMIS corrects only the origin between the two arms. You should do this type of calibration more frequently, based on probe calibration procedures.

Entry Name: OriginMode

Entry Type: Whole Number specifying 0 (Orientation and origin) or 1 (Origin only). Default value is 0.

User permission is required to change entry