Current Help System: PC-DMIS Settings Editor (View Core Help)

### TCPIP Send Port Arm (1-4)

Provides the port number of the TCP/IP address for the given arm (1-4) arm to the current (master) computer. Values can be provided for Arm 1-4 respectively. This value is only used when ConnectionTypeArm(1-4) for the relevant arm is set to 1(Remote Connection) and this is the Master computer set with a value of 1 for Mode.

Entry Name: TCPIPSendPortArm(1-4)

Entry Type: Character String specifying the TCP/IP port. Default value is None ( ).

User permission is required to change entry.