Current Help System: PC-DMIS Settings Editor (View Core Help)

### Section Axis

Specifies the axis to be used with Section scans. The available axes are X, Y, and Z. The cut plane that your probe will crisscross will be parallel to this axis.

Entry Name: Section Axis

Entry Type: Whole Number specifying axis number. Default value is 0.

User permission is required to change entry

Axis Key

0 | X
1 | Y
2 | Z
3 | None